v1
GLOBAL_SIGNAL_SINGLE_POINT_ASSIGNMENT,,,
GLOBAL_SIGNAL_SINGLE_POINT_ASSIGNMENT,aurora_8b10b_v5_2:aurora_module_i|MGT_alt4gxb:MGT_0|rx_coreclk_in[0],Global Clock,
GLOBAL_SIGNAL_SINGLE_POINT_ASSIGNMENT,aurora_8b10b_v5_2:aurora_module_i|MGT_alt4gxb:MGT_0|tx_coreclk_in[0],Periphery Clock,
GLOBAL_SIGNAL_SINGLE_POINT_ASSIGNMENT,aurora_8b10b_v5_2_RESET_LOGIC:reset_logic_i|GT_RESET_OUT,Global Clock,
GLOBAL_SIGNAL_SINGLE_POINT_ASSIGNMENT,altera_internal_jtag~TCKUTAP,Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_offload_buffer_mgr:\stp_non_zero_depth_offload_gen:stp_offload_buff_mgr_inst|lpm_shiftreg:info_data_shift_out|dffs[0],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_offload_buffer_mgr:\stp_non_zero_depth_offload_gen:stp_offload_buff_mgr_inst|lpm_shiftreg:status_data_shift_out|dffs[0],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_offload_buffer_mgr:\stp_non_zero_depth_offload_gen:stp_offload_buff_mgr_inst|lpm_shiftreg:info_data_shift_out|dffs[1],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_offload_buffer_mgr:\stp_non_zero_depth_offload_gen:stp_offload_buff_mgr_inst|lpm_shiftreg:status_data_shift_out|dffs[1],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_buffer_manager:sld_buffer_manager_inst|counter[11],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_buffer_manager:sld_buffer_manager_inst|counter[9],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_buffer_manager:sld_buffer_manager_inst|counter[10],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_buffer_manager:sld_buffer_manager_inst|counter[8],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_buffer_manager:sld_buffer_manager_inst|counter[6],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_buffer_manager:sld_buffer_manager_inst|counter[7],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_buffer_manager:sld_buffer_manager_inst|counter[2],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_buffer_manager:sld_buffer_manager_inst|counter[0],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_buffer_manager:sld_buffer_manager_inst|counter[1],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_buffer_manager:sld_buffer_manager_inst|counter[5],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_buffer_manager:sld_buffer_manager_inst|counter[3],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_buffer_manager:sld_buffer_manager_inst|counter[4],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_offload_buffer_mgr:\stp_non_zero_depth_offload_gen:stp_offload_buff_mgr_inst|lpm_shiftreg:info_data_shift_out|dffs[2],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_buffer_manager:sld_buffer_manager_inst|last_buffer_write_address_sig[0],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_offload_buffer_mgr:\stp_non_zero_depth_offload_gen:stp_offload_buff_mgr_inst|lpm_shiftreg:status_data_shift_out|dffs[2],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_buffer_manager:sld_buffer_manager_inst|\buffer_manager:next_address[0],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_buffer_manager:sld_buffer_manager_inst|\buffer_manager:next_address[10],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_buffer_manager:sld_buffer_manager_inst|\buffer_manager:next_address[9],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_buffer_manager:sld_buffer_manager_inst|\buffer_manager:next_address[8],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_buffer_manager:sld_buffer_manager_inst|\buffer_manager:next_address[7],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_buffer_manager:sld_buffer_manager_inst|\buffer_manager:next_address[6],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_buffer_manager:sld_buffer_manager_inst|\buffer_manager:next_address[5],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_buffer_manager:sld_buffer_manager_inst|\buffer_manager:next_address[4],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_buffer_manager:sld_buffer_manager_inst|\buffer_manager:next_address[3],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_buffer_manager:sld_buffer_manager_inst|\buffer_manager:next_address[2],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_buffer_manager:sld_buffer_manager_inst|\buffer_manager:next_address[1],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_offload_buffer_mgr:\stp_non_zero_depth_offload_gen:stp_offload_buff_mgr_inst|lpm_shiftreg:info_data_shift_out|dffs[3],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_buffer_manager:sld_buffer_manager_inst|last_buffer_write_address_sig[1],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_offload_buffer_mgr:\stp_non_zero_depth_offload_gen:stp_offload_buff_mgr_inst|lpm_shiftreg:status_data_shift_out|dffs[3],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_offload_buffer_mgr:\stp_non_zero_depth_offload_gen:stp_offload_buff_mgr_inst|lpm_shiftreg:info_data_shift_out|dffs[4],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_buffer_manager:sld_buffer_manager_inst|last_buffer_write_address_sig[2],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_offload_buffer_mgr:\stp_non_zero_depth_offload_gen:stp_offload_buff_mgr_inst|lpm_shiftreg:status_data_shift_out|dffs[4],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_offload_buffer_mgr:\stp_non_zero_depth_offload_gen:stp_offload_buff_mgr_inst|lpm_shiftreg:info_data_shift_out|dffs[5],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_buffer_manager:sld_buffer_manager_inst|last_buffer_write_address_sig[3],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_buffer_manager:sld_buffer_manager_inst|\buffer_manager:last_trigger_address_var[0],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_offload_buffer_mgr:\stp_non_zero_depth_offload_gen:stp_offload_buff_mgr_inst|lpm_shiftreg:status_data_shift_out|dffs[5],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_offload_buffer_mgr:\stp_non_zero_depth_offload_gen:stp_offload_buff_mgr_inst|lpm_shiftreg:info_data_shift_out|dffs[6],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_buffer_manager:sld_buffer_manager_inst|last_buffer_write_address_sig[4],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_buffer_manager:sld_buffer_manager_inst|\buffer_manager:last_trigger_address_var[1],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_offload_buffer_mgr:\stp_non_zero_depth_offload_gen:stp_offload_buff_mgr_inst|lpm_shiftreg:status_data_shift_out|dffs[6],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_offload_buffer_mgr:\stp_non_zero_depth_offload_gen:stp_offload_buff_mgr_inst|lpm_shiftreg:info_data_shift_out|dffs[7],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_buffer_manager:sld_buffer_manager_inst|last_buffer_write_address_sig[5],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_buffer_manager:sld_buffer_manager_inst|\buffer_manager:last_trigger_address_var[2],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_offload_buffer_mgr:\stp_non_zero_depth_offload_gen:stp_offload_buff_mgr_inst|lpm_shiftreg:status_data_shift_out|dffs[7],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_offload_buffer_mgr:\stp_non_zero_depth_offload_gen:stp_offload_buff_mgr_inst|lpm_shiftreg:info_data_shift_out|dffs[8],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_buffer_manager:sld_buffer_manager_inst|last_buffer_write_address_sig[6],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_buffer_manager:sld_buffer_manager_inst|\buffer_manager:last_trigger_address_var[3],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_offload_buffer_mgr:\stp_non_zero_depth_offload_gen:stp_offload_buff_mgr_inst|lpm_shiftreg:status_data_shift_out|dffs[8],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_offload_buffer_mgr:\stp_non_zero_depth_offload_gen:stp_offload_buff_mgr_inst|lpm_shiftreg:info_data_shift_out|dffs[9],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_buffer_manager:sld_buffer_manager_inst|last_buffer_write_address_sig[7],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_buffer_manager:sld_buffer_manager_inst|\buffer_manager:last_trigger_address_var[4],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_offload_buffer_mgr:\stp_non_zero_depth_offload_gen:stp_offload_buff_mgr_inst|lpm_shiftreg:status_data_shift_out|dffs[9],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_offload_buffer_mgr:\stp_non_zero_depth_offload_gen:stp_offload_buff_mgr_inst|lpm_shiftreg:info_data_shift_out|dffs[10],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_buffer_manager:sld_buffer_manager_inst|last_buffer_write_address_sig[8],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_buffer_manager:sld_buffer_manager_inst|\buffer_manager:last_trigger_address_var[5],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_offload_buffer_mgr:\stp_non_zero_depth_offload_gen:stp_offload_buff_mgr_inst|lpm_shiftreg:status_data_shift_out|dffs[10],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_offload_buffer_mgr:\stp_non_zero_depth_offload_gen:stp_offload_buff_mgr_inst|lpm_shiftreg:info_data_shift_out|dffs[11],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_buffer_manager:sld_buffer_manager_inst|last_buffer_write_address_sig[9],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_buffer_manager:sld_buffer_manager_inst|\buffer_manager:last_trigger_address_var[6],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_offload_buffer_mgr:\stp_non_zero_depth_offload_gen:stp_offload_buff_mgr_inst|lpm_shiftreg:status_data_shift_out|dffs[11],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_offload_buffer_mgr:\stp_non_zero_depth_offload_gen:stp_offload_buff_mgr_inst|lpm_shiftreg:info_data_shift_out|dffs[12],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_buffer_manager:sld_buffer_manager_inst|last_buffer_write_address_sig[10],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_buffer_manager:sld_buffer_manager_inst|\buffer_manager:last_trigger_address_var[7],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_offload_buffer_mgr:\stp_non_zero_depth_offload_gen:stp_offload_buff_mgr_inst|lpm_shiftreg:status_data_shift_out|dffs[12],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_offload_buffer_mgr:\stp_non_zero_depth_offload_gen:stp_offload_buff_mgr_inst|lpm_shiftreg:info_data_shift_out|dffs[13],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_buffer_manager:sld_buffer_manager_inst|\buffer_manager:last_trigger_address_var[8],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_offload_buffer_mgr:\stp_non_zero_depth_offload_gen:stp_offload_buff_mgr_inst|lpm_shiftreg:status_data_shift_out|dffs[13],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_offload_buffer_mgr:\stp_non_zero_depth_offload_gen:stp_offload_buff_mgr_inst|lpm_shiftreg:info_data_shift_out|dffs[14],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_buffer_manager:sld_buffer_manager_inst|\buffer_manager:last_trigger_address_var[9],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_offload_buffer_mgr:\stp_non_zero_depth_offload_gen:stp_offload_buff_mgr_inst|lpm_shiftreg:status_data_shift_out|dffs[14],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_offload_buffer_mgr:\stp_non_zero_depth_offload_gen:stp_offload_buff_mgr_inst|lpm_shiftreg:info_data_shift_out|dffs[15],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_buffer_manager:sld_buffer_manager_inst|\buffer_manager:last_trigger_address_var[10],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_offload_buffer_mgr:\stp_non_zero_depth_offload_gen:stp_offload_buff_mgr_inst|lpm_shiftreg:status_data_shift_out|dffs[15],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_offload_buffer_mgr:\stp_non_zero_depth_offload_gen:stp_offload_buff_mgr_inst|lpm_shiftreg:info_data_shift_out|dffs[16],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_offload_buffer_mgr:\stp_non_zero_depth_offload_gen:stp_offload_buff_mgr_inst|lpm_shiftreg:status_data_shift_out|dffs[16],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_offload_buffer_mgr:\stp_non_zero_depth_offload_gen:stp_offload_buff_mgr_inst|lpm_shiftreg:info_data_shift_out|dffs[17],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_offload_buffer_mgr:\stp_non_zero_depth_offload_gen:stp_offload_buff_mgr_inst|lpm_shiftreg:status_data_shift_out|dffs[17],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_offload_buffer_mgr:\stp_non_zero_depth_offload_gen:stp_offload_buff_mgr_inst|lpm_shiftreg:info_data_shift_out|dffs[18],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_offload_buffer_mgr:\stp_non_zero_depth_offload_gen:stp_offload_buff_mgr_inst|lpm_shiftreg:status_data_shift_out|dffs[18],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_offload_buffer_mgr:\stp_non_zero_depth_offload_gen:stp_offload_buff_mgr_inst|lpm_shiftreg:info_data_shift_out|dffs[19],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_offload_buffer_mgr:\stp_non_zero_depth_offload_gen:stp_offload_buff_mgr_inst|lpm_shiftreg:status_data_shift_out|dffs[19],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_offload_buffer_mgr:\stp_non_zero_depth_offload_gen:stp_offload_buff_mgr_inst|lpm_shiftreg:info_data_shift_out|dffs[20],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_offload_buffer_mgr:\stp_non_zero_depth_offload_gen:stp_offload_buff_mgr_inst|lpm_shiftreg:status_data_shift_out|dffs[20],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_offload_buffer_mgr:\stp_non_zero_depth_offload_gen:stp_offload_buff_mgr_inst|lpm_shiftreg:info_data_shift_out|dffs[21],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_offload_buffer_mgr:\stp_non_zero_depth_offload_gen:stp_offload_buff_mgr_inst|lpm_shiftreg:status_data_shift_out|dffs[21],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_offload_buffer_mgr:\stp_non_zero_depth_offload_gen:stp_offload_buff_mgr_inst|lpm_shiftreg:info_data_shift_out|dffs[22],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_offload_buffer_mgr:\stp_non_zero_depth_offload_gen:stp_offload_buff_mgr_inst|lpm_shiftreg:ram_data_shift_out|dffs[0],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_offload_buffer_mgr:\stp_non_zero_depth_offload_gen:stp_offload_buff_mgr_inst|lpm_shiftreg:ram_data_shift_out|dffs[1],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_offload_buffer_mgr:\stp_non_zero_depth_offload_gen:stp_offload_buff_mgr_inst|lpm_shiftreg:ram_data_shift_out|dffs[2],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_offload_buffer_mgr:\stp_non_zero_depth_offload_gen:stp_offload_buff_mgr_inst|lpm_shiftreg:ram_data_shift_out|dffs[3],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_offload_buffer_mgr:\stp_non_zero_depth_offload_gen:stp_offload_buff_mgr_inst|lpm_shiftreg:ram_data_shift_out|dffs[4],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_offload_buffer_mgr:\stp_non_zero_depth_offload_gen:stp_offload_buff_mgr_inst|lpm_shiftreg:ram_data_shift_out|dffs[5],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_offload_buffer_mgr:\stp_non_zero_depth_offload_gen:stp_offload_buff_mgr_inst|lpm_shiftreg:ram_data_shift_out|dffs[6],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_offload_buffer_mgr:\stp_non_zero_depth_offload_gen:stp_offload_buff_mgr_inst|lpm_shiftreg:ram_data_shift_out|dffs[7],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_offload_buffer_mgr:\stp_non_zero_depth_offload_gen:stp_offload_buff_mgr_inst|lpm_shiftreg:ram_data_shift_out|dffs[8],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_offload_buffer_mgr:\stp_non_zero_depth_offload_gen:stp_offload_buff_mgr_inst|lpm_shiftreg:ram_data_shift_out|dffs[9],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_offload_buffer_mgr:\stp_non_zero_depth_offload_gen:stp_offload_buff_mgr_inst|lpm_shiftreg:ram_data_shift_out|dffs[10],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_offload_buffer_mgr:\stp_non_zero_depth_offload_gen:stp_offload_buff_mgr_inst|lpm_shiftreg:ram_data_shift_out|dffs[11],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_offload_buffer_mgr:\stp_non_zero_depth_offload_gen:stp_offload_buff_mgr_inst|lpm_shiftreg:ram_data_shift_out|dffs[12],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_offload_buffer_mgr:\stp_non_zero_depth_offload_gen:stp_offload_buff_mgr_inst|lpm_shiftreg:ram_data_shift_out|dffs[13],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_offload_buffer_mgr:\stp_non_zero_depth_offload_gen:stp_offload_buff_mgr_inst|lpm_shiftreg:ram_data_shift_out|dffs[14],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_offload_buffer_mgr:\stp_non_zero_depth_offload_gen:stp_offload_buff_mgr_inst|lpm_shiftreg:ram_data_shift_out|dffs[15],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_offload_buffer_mgr:\stp_non_zero_depth_offload_gen:stp_offload_buff_mgr_inst|lpm_shiftreg:ram_data_shift_out|dffs[16],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_offload_buffer_mgr:\stp_non_zero_depth_offload_gen:stp_offload_buff_mgr_inst|lpm_shiftreg:ram_data_shift_out|dffs[17],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_offload_buffer_mgr:\stp_non_zero_depth_offload_gen:stp_offload_buff_mgr_inst|lpm_shiftreg:ram_data_shift_out|dffs[18],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_offload_buffer_mgr:\stp_non_zero_depth_offload_gen:stp_offload_buff_mgr_inst|lpm_shiftreg:ram_data_shift_out|dffs[19],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_offload_buffer_mgr:\stp_non_zero_depth_offload_gen:stp_offload_buff_mgr_inst|lpm_shiftreg:ram_data_shift_out|dffs[20],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_offload_buffer_mgr:\stp_non_zero_depth_offload_gen:stp_offload_buff_mgr_inst|lpm_shiftreg:ram_data_shift_out|dffs[21],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_offload_buffer_mgr:\stp_non_zero_depth_offload_gen:stp_offload_buff_mgr_inst|lpm_shiftreg:ram_data_shift_out|dffs[22],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_offload_buffer_mgr:\stp_non_zero_depth_offload_gen:stp_offload_buff_mgr_inst|lpm_shiftreg:ram_data_shift_out|dffs[23],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_offload_buffer_mgr:\stp_non_zero_depth_offload_gen:stp_offload_buff_mgr_inst|lpm_shiftreg:ram_data_shift_out|dffs[24],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_offload_buffer_mgr:\stp_non_zero_depth_offload_gen:stp_offload_buff_mgr_inst|lpm_shiftreg:ram_data_shift_out|dffs[25],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_offload_buffer_mgr:\stp_non_zero_depth_offload_gen:stp_offload_buff_mgr_inst|lpm_shiftreg:ram_data_shift_out|dffs[26],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_offload_buffer_mgr:\stp_non_zero_depth_offload_gen:stp_offload_buff_mgr_inst|lpm_shiftreg:ram_data_shift_out|dffs[27],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_offload_buffer_mgr:\stp_non_zero_depth_offload_gen:stp_offload_buff_mgr_inst|lpm_shiftreg:ram_data_shift_out|dffs[28],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_offload_buffer_mgr:\stp_non_zero_depth_offload_gen:stp_offload_buff_mgr_inst|lpm_shiftreg:ram_data_shift_out|dffs[29],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_offload_buffer_mgr:\stp_non_zero_depth_offload_gen:stp_offload_buff_mgr_inst|lpm_shiftreg:ram_data_shift_out|dffs[30],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_offload_buffer_mgr:\stp_non_zero_depth_offload_gen:stp_offload_buff_mgr_inst|lpm_shiftreg:ram_data_shift_out|dffs[31],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_offload_buffer_mgr:\stp_non_zero_depth_offload_gen:stp_offload_buff_mgr_inst|lpm_shiftreg:ram_data_shift_out|dffs[32],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_offload_buffer_mgr:\stp_non_zero_depth_offload_gen:stp_offload_buff_mgr_inst|lpm_shiftreg:ram_data_shift_out|dffs[33],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_offload_buffer_mgr:\stp_non_zero_depth_offload_gen:stp_offload_buff_mgr_inst|lpm_shiftreg:ram_data_shift_out|dffs[34],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_offload_buffer_mgr:\stp_non_zero_depth_offload_gen:stp_offload_buff_mgr_inst|lpm_shiftreg:ram_data_shift_out|dffs[35],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_offload_buffer_mgr:\stp_non_zero_depth_offload_gen:stp_offload_buff_mgr_inst|lpm_shiftreg:ram_data_shift_out|dffs[36],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_offload_buffer_mgr:\stp_non_zero_depth_offload_gen:stp_offload_buff_mgr_inst|lpm_shiftreg:ram_data_shift_out|dffs[37],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|bypass_reg_out,Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|lpm_shiftreg:segment_offset_config_deserialize|dffs[0],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_buffer_manager:sld_buffer_manager_inst|\buffer_manager:collecting_post_data_var,Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_buffer_manager:sld_buffer_manager_inst|is_buffer_wrapped_once_sig,Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|lpm_shiftreg:segment_offset_config_deserialize|dffs[1],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_buffer_manager:sld_buffer_manager_inst|\buffer_manager:done,Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_buffer_manager:sld_buffer_manager_inst|\buffer_manager:is_buffer_wrapped,Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_ela_control:ela_control|sld_ela_trigger_flow_mgr:\builtin:ela_trigger_flow_mgr_entity|last_level_delayed,Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_ela_control:ela_control|sld_ela_trigger_flow_mgr:\builtin:ela_trigger_flow_mgr_entity|lpm_shiftreg:trigger_config_deserialize|dffs[0],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_buffer_manager:sld_buffer_manager_inst|final_trigger_set,Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_buffer_manager:sld_buffer_manager_inst|modified_post_count[11],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_buffer_manager:sld_buffer_manager_inst|modified_post_count[9],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_buffer_manager:sld_buffer_manager_inst|modified_post_count[10],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_buffer_manager:sld_buffer_manager_inst|modified_post_count[8],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_buffer_manager:sld_buffer_manager_inst|modified_post_count[6],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_buffer_manager:sld_buffer_manager_inst|modified_post_count[7],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_buffer_manager:sld_buffer_manager_inst|modified_post_count[2],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_buffer_manager:sld_buffer_manager_inst|modified_post_count[0],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_buffer_manager:sld_buffer_manager_inst|modified_post_count[1],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_buffer_manager:sld_buffer_manager_inst|modified_post_count[5],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_buffer_manager:sld_buffer_manager_inst|modified_post_count[3],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_buffer_manager:sld_buffer_manager_inst|modified_post_count[4],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_buffer_manager:sld_buffer_manager_inst|\buffer_manager:base_address[0],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|lpm_shiftreg:segment_offset_config_deserialize|dffs[2],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_ela_control:ela_control|lpm_shiftreg:trigger_config_deserialize|dffs[0],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_ela_control:ela_control|run,Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_ela_control:ela_control|sld_ela_trigger_flow_mgr:\builtin:ela_trigger_flow_mgr_entity|lpm_shiftreg:trigger_config_deserialize|dffs[1],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|lpm_shiftreg:segment_offset_config_deserialize|dffs[10],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|lpm_shiftreg:segment_offset_config_deserialize|dffs[9],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|lpm_shiftreg:segment_offset_config_deserialize|dffs[8],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|lpm_shiftreg:segment_offset_config_deserialize|dffs[7],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|lpm_shiftreg:segment_offset_config_deserialize|dffs[6],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|lpm_shiftreg:segment_offset_config_deserialize|dffs[5],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|lpm_shiftreg:segment_offset_config_deserialize|dffs[4],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|lpm_shiftreg:segment_offset_config_deserialize|dffs[3],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_buffer_manager:sld_buffer_manager_inst|\buffer_manager:segment_shift_var,Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_ela_control:ela_control|lpm_shiftreg:trigger_config_deserialize|dffs[1],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_ela_control:ela_control|sld_ela_basic_multi_level_trigger:\basic_multi_level_mbpm_trigger_gen:multi_level_mbpm|lpm_shiftreg:trigger_condition_deserialize|dffs[0],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_ela_control:ela_control|sld_ela_basic_multi_level_trigger:\basic_multi_level_mbpm_trigger_gen:multi_level_mbpm|lpm_shiftreg:trigger_condition_deserialize|dffs[2],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_ela_control:ela_control|sld_ela_basic_multi_level_trigger:\basic_multi_level_mbpm_trigger_gen:multi_level_mbpm|lpm_shiftreg:trigger_condition_deserialize|dffs[1],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_ela_control:ela_control|sld_ela_trigger_flow_mgr:\builtin:ela_trigger_flow_mgr_entity|lpm_shiftreg:trigger_config_deserialize|dffs[2],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_ela_control:ela_control|lpm_shiftreg:trigger_config_deserialize|dffs[2],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_ela_control:ela_control|sld_ela_trigger_flow_mgr:\builtin:ela_trigger_flow_mgr_entity|lpm_shiftreg:trigger_config_deserialize|dffs[3],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_ela_control:ela_control|lpm_shiftreg:trigger_config_deserialize|dffs[3],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_ela_control:ela_control|sld_ela_trigger_flow_mgr:\builtin:ela_trigger_flow_mgr_entity|lpm_shiftreg:trigger_config_deserialize|dffs[4],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_ela_control:ela_control|sld_ela_trigger_flow_mgr:\builtin:ela_trigger_flow_mgr_entity|lpm_shiftreg:trigger_config_deserialize|dffs[5],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_ela_control:ela_control|sld_ela_trigger_flow_mgr:\builtin:ela_trigger_flow_mgr_entity|lpm_shiftreg:trigger_config_deserialize|dffs[6],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_ela_control:ela_control|sld_ela_trigger_flow_mgr:\builtin:ela_trigger_flow_mgr_entity|lpm_shiftreg:trigger_config_deserialize|dffs[7],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_ela_control:ela_control|sld_ela_trigger_flow_mgr:\builtin:ela_trigger_flow_mgr_entity|lpm_shiftreg:trigger_config_deserialize|dffs[8],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_ela_control:ela_control|sld_ela_trigger_flow_mgr:\builtin:ela_trigger_flow_mgr_entity|lpm_shiftreg:trigger_config_deserialize|dffs[9],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_offload_buffer_mgr:\stp_non_zero_depth_offload_gen:stp_offload_buff_mgr_inst|lpm_shiftreg:status_data_shift_out|dffs[22],Global Clock,
GLOBAL_SIGNAL_POINT_TO_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|sld_offload_buffer_mgr:\stp_non_zero_depth_offload_gen:stp_offload_buff_mgr_inst|lpm_shiftreg:ram_data_shift_out|dffs[38],Global Clock,
GLOBAL_SIGNAL_SINGLE_POINT_ASSIGNMENT,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|reset_all,Off,
GLOBAL_SIGNAL_SINGLE_POINT_ASSIGNMENT,INIT_CLK,Global Clock,
RAM_PACKING,0,M4K,4,4,SimpleDual,0,0,111001000100,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|altsyncram:\stp_non_zero_ram_gen:stp_buffer_ram|altsyncram_6p14:auto_generated|ram_block1a0,
RAM_PACKING,0,M4K,4,4,SimpleDual,0,1,111001000100,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|altsyncram:\stp_non_zero_ram_gen:stp_buffer_ram|altsyncram_6p14:auto_generated|ram_block1a1,
RAM_PACKING,0,M4K,4,4,SimpleDual,0,2,111001000100,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|altsyncram:\stp_non_zero_ram_gen:stp_buffer_ram|altsyncram_6p14:auto_generated|ram_block1a2,
RAM_PACKING,0,M4K,4,4,SimpleDual,0,3,111001000100,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|altsyncram:\stp_non_zero_ram_gen:stp_buffer_ram|altsyncram_6p14:auto_generated|ram_block1a3,
RAM_PACKING,1,M4K,4,4,SimpleDual,0,0,111001000100,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|altsyncram:\stp_non_zero_ram_gen:stp_buffer_ram|altsyncram_6p14:auto_generated|ram_block1a4,
RAM_PACKING,1,M4K,4,4,SimpleDual,0,1,111001000100,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|altsyncram:\stp_non_zero_ram_gen:stp_buffer_ram|altsyncram_6p14:auto_generated|ram_block1a5,
RAM_PACKING,1,M4K,4,4,SimpleDual,0,2,111001000100,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|altsyncram:\stp_non_zero_ram_gen:stp_buffer_ram|altsyncram_6p14:auto_generated|ram_block1a6,
RAM_PACKING,1,M4K,4,4,SimpleDual,0,3,111001000100,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|altsyncram:\stp_non_zero_ram_gen:stp_buffer_ram|altsyncram_6p14:auto_generated|ram_block1a7,
RAM_PACKING,2,M4K,4,4,SimpleDual,0,0,111001000100,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|altsyncram:\stp_non_zero_ram_gen:stp_buffer_ram|altsyncram_6p14:auto_generated|ram_block1a8,
RAM_PACKING,2,M4K,4,4,SimpleDual,0,1,111001000100,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|altsyncram:\stp_non_zero_ram_gen:stp_buffer_ram|altsyncram_6p14:auto_generated|ram_block1a9,
RAM_PACKING,2,M4K,4,4,SimpleDual,0,2,111001000100,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|altsyncram:\stp_non_zero_ram_gen:stp_buffer_ram|altsyncram_6p14:auto_generated|ram_block1a10,
RAM_PACKING,2,M4K,4,4,SimpleDual,0,3,111001000100,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|altsyncram:\stp_non_zero_ram_gen:stp_buffer_ram|altsyncram_6p14:auto_generated|ram_block1a11,
RAM_PACKING,3,M4K,4,4,SimpleDual,0,0,111001000100,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|altsyncram:\stp_non_zero_ram_gen:stp_buffer_ram|altsyncram_6p14:auto_generated|ram_block1a12,
RAM_PACKING,3,M4K,4,4,SimpleDual,0,1,111001000100,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|altsyncram:\stp_non_zero_ram_gen:stp_buffer_ram|altsyncram_6p14:auto_generated|ram_block1a13,
RAM_PACKING,3,M4K,4,4,SimpleDual,0,2,111001000100,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|altsyncram:\stp_non_zero_ram_gen:stp_buffer_ram|altsyncram_6p14:auto_generated|ram_block1a14,
RAM_PACKING,3,M4K,4,4,SimpleDual,0,3,111001000100,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|altsyncram:\stp_non_zero_ram_gen:stp_buffer_ram|altsyncram_6p14:auto_generated|ram_block1a15,
RAM_PACKING,4,M4K,4,4,SimpleDual,0,0,111001000100,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|altsyncram:\stp_non_zero_ram_gen:stp_buffer_ram|altsyncram_6p14:auto_generated|ram_block1a16,
RAM_PACKING,4,M4K,4,4,SimpleDual,0,1,111001000100,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|altsyncram:\stp_non_zero_ram_gen:stp_buffer_ram|altsyncram_6p14:auto_generated|ram_block1a17,
RAM_PACKING,4,M4K,4,4,SimpleDual,0,2,111001000100,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|altsyncram:\stp_non_zero_ram_gen:stp_buffer_ram|altsyncram_6p14:auto_generated|ram_block1a18,
RAM_PACKING,4,M4K,4,4,SimpleDual,0,3,111001000100,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|altsyncram:\stp_non_zero_ram_gen:stp_buffer_ram|altsyncram_6p14:auto_generated|ram_block1a19,
RAM_PACKING,5,M4K,4,4,SimpleDual,0,0,111001000100,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|altsyncram:\stp_non_zero_ram_gen:stp_buffer_ram|altsyncram_6p14:auto_generated|ram_block1a20,
RAM_PACKING,5,M4K,4,4,SimpleDual,0,1,111001000100,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|altsyncram:\stp_non_zero_ram_gen:stp_buffer_ram|altsyncram_6p14:auto_generated|ram_block1a21,
RAM_PACKING,5,M4K,4,4,SimpleDual,0,2,111001000100,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|altsyncram:\stp_non_zero_ram_gen:stp_buffer_ram|altsyncram_6p14:auto_generated|ram_block1a22,
RAM_PACKING,5,M4K,4,4,SimpleDual,0,3,111001000100,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|altsyncram:\stp_non_zero_ram_gen:stp_buffer_ram|altsyncram_6p14:auto_generated|ram_block1a23,
RAM_PACKING,6,M4K,4,4,SimpleDual,0,0,111001000100,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|altsyncram:\stp_non_zero_ram_gen:stp_buffer_ram|altsyncram_6p14:auto_generated|ram_block1a24,
RAM_PACKING,6,M4K,4,4,SimpleDual,0,1,111001000100,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|altsyncram:\stp_non_zero_ram_gen:stp_buffer_ram|altsyncram_6p14:auto_generated|ram_block1a25,
RAM_PACKING,6,M4K,4,4,SimpleDual,0,2,111001000100,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|altsyncram:\stp_non_zero_ram_gen:stp_buffer_ram|altsyncram_6p14:auto_generated|ram_block1a26,
RAM_PACKING,6,M4K,4,4,SimpleDual,0,3,111001000100,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|altsyncram:\stp_non_zero_ram_gen:stp_buffer_ram|altsyncram_6p14:auto_generated|ram_block1a27,
RAM_PACKING,7,M4K,4,4,SimpleDual,0,0,111001000100,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|altsyncram:\stp_non_zero_ram_gen:stp_buffer_ram|altsyncram_6p14:auto_generated|ram_block1a28,
RAM_PACKING,7,M4K,4,4,SimpleDual,0,1,111001000100,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|altsyncram:\stp_non_zero_ram_gen:stp_buffer_ram|altsyncram_6p14:auto_generated|ram_block1a29,
RAM_PACKING,7,M4K,4,4,SimpleDual,0,2,111001000100,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|altsyncram:\stp_non_zero_ram_gen:stp_buffer_ram|altsyncram_6p14:auto_generated|ram_block1a30,
RAM_PACKING,7,M4K,4,4,SimpleDual,0,3,111001000100,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|altsyncram:\stp_non_zero_ram_gen:stp_buffer_ram|altsyncram_6p14:auto_generated|ram_block1a31,
RAM_PACKING,8,M4K,4,4,SimpleDual,0,0,111001000100,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|altsyncram:\stp_non_zero_ram_gen:stp_buffer_ram|altsyncram_6p14:auto_generated|ram_block1a32,
RAM_PACKING,8,M4K,4,4,SimpleDual,0,1,111001000100,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|altsyncram:\stp_non_zero_ram_gen:stp_buffer_ram|altsyncram_6p14:auto_generated|ram_block1a33,
RAM_PACKING,8,M4K,4,4,SimpleDual,0,2,111001000100,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|altsyncram:\stp_non_zero_ram_gen:stp_buffer_ram|altsyncram_6p14:auto_generated|ram_block1a34,
RAM_PACKING,8,M4K,4,4,SimpleDual,0,3,111001000100,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|altsyncram:\stp_non_zero_ram_gen:stp_buffer_ram|altsyncram_6p14:auto_generated|ram_block1a35,
RAM_PACKING,9,M4K,4,4,SimpleDual,0,0,111001000100,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|altsyncram:\stp_non_zero_ram_gen:stp_buffer_ram|altsyncram_6p14:auto_generated|ram_block1a36,
RAM_PACKING,9,M4K,4,4,SimpleDual,0,1,111001000100,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|altsyncram:\stp_non_zero_ram_gen:stp_buffer_ram|altsyncram_6p14:auto_generated|ram_block1a37,
RAM_PACKING,9,M4K,4,4,SimpleDual,0,2,111001000100,sld_signaltap:auto_signaltap_0|sld_signaltap_impl:sld_signaltap_body|altsyncram:\stp_non_zero_ram_gen:stp_buffer_ram|altsyncram_6p14:auto_generated|ram_block1a38,
IO_RULES,NUM_PINS_NOT_EXCEED_LOC_AVAILABLE,PASS,IO_000001,Capacity Checks,Number of pins in an I/O bank should not exceed the number of locations available.,Critical,0 such failures found.,,I/O,,
IO_RULES,NUM_CLKS_NOT_EXCEED_CLKS_AVAILABLE,INAPPLICABLE,IO_000002,Capacity Checks,Number of clocks in an I/O bank should not exceed the number of clocks available.,Critical,No Global Signal assignments found.,,I/O,,
IO_RULES,NUM_VREF_NOT_EXCEED_LOC_AVAILABLE,PASS,IO_000003,Capacity Checks,Number of pins in a Vrefgroup should not exceed the number of locations available.,Critical,0 such failures found.,,I/O,,
IO_RULES,IO_BANK_SUPPORT_VCCIO,INAPPLICABLE,IO_000004,Voltage Compatibility Checks,The I/O bank should support the requested VCCIO.,Critical,No IOBANK_VCCIO assignments found.,,I/O,,
IO_RULES,IO_BANK_NOT_HAVE_COMPETING_VREF,INAPPLICABLE,IO_000005,Voltage Compatibility Checks,The I/O bank should not have competing VREF values.,Critical,No VREF I/O Standard assignments found.,,I/O,,
IO_RULES,IO_BANK_NOT_HAVE_COMPETING_VCCIO,PASS,IO_000006,Voltage Compatibility Checks,The I/O bank should not have competing VCCIO values.,Critical,0 such failures found.,,I/O,,
IO_RULES,CHECK_UNAVAILABLE_LOC,PASS,IO_000007,Valid Location Checks,Checks for unavailable locations.,Critical,0 such failures found.,,I/O,,
IO_RULES,CHECK_RESERVED_LOC,INAPPLICABLE,IO_000008,Valid Location Checks,Checks for reserved locations.,Critical,No reserved LogicLock region found.,,I/O,,
IO_RULES,LOC_SUPPORT_IO_STD,PASS,IO_000009,I/O Properties Checks for One I/O,The location should support the requested I/O standard.,Critical,0 such failures found.,,I/O,,
IO_RULES,LOC_SUPPORT_IO_DIR,PASS,IO_000010,I/O Properties Checks for One I/O,The location should support the requested I/O direction.,Critical,0 such failures found.,,I/O,,
IO_RULES,LOC_SUPPORT_CURRENT_STRENGTH,INAPPLICABLE,IO_000011,I/O Properties Checks for One I/O,The location should support the requested Current Strength.,Critical,No Current Strength assignments found.,,I/O,,
IO_RULES,LOC_SUPPORT_OCT_VALUE,PASS,IO_000012,I/O Properties Checks for One I/O,The location should support the requested On Chip Termination value.,Critical,0 such failures found.,,I/O,,
IO_RULES,LOC_SUPPORT_BUS_HOLD_VALUE,INAPPLICABLE,IO_000013,I/O Properties Checks for One I/O,The location should support the requested Bus Hold value.,Critical,No Enable Bus-Hold Circuitry assignments found.,,I/O,,
IO_RULES,LOC_SUPPORT_WEAK_PULL_UP_VALUE,INAPPLICABLE,IO_000014,I/O Properties Checks for One I/O,The location should support the requested Weak Pull Up value.,Critical,No Weak Pull-Up Resistor assignments found.,,I/O,,
IO_RULES,LOC_SUPPORT_PCI_CLAMP_DIODE,INAPPLICABLE,IO_000015,I/O Properties Checks for One I/O,The location should support the requested PCI Clamp Diode.,Critical,No Clamping Diode assignments found.,,I/O,,
IO_RULES,IO_STD_SUPPORT_CURRENT_STRENGTH,INAPPLICABLE,IO_000018,I/O Properties Checks for One I/O,The I/O standard should support the requested Current Strength.,Critical,No Current Strength assignments found.,,I/O,,
IO_RULES,IO_STD_SUPPORT_OCT_VALUE,PASS,IO_000019,I/O Properties Checks for One I/O,The I/O standard should support the requested On Chip Termination value.,Critical,0 such failures found.,,I/O,,
IO_RULES,IO_STD_SUPPORT_PCI_CLAMP_DIODE,INAPPLICABLE,IO_000020,I/O Properties Checks for One I/O,The I/O standard should support the requested PCI Clamp Diode.,Critical,No Clamping Diode assignments found.,,I/O,,
IO_RULES,IO_STD_SUPPORT_WEAK_PULL_UP_VALUE,INAPPLICABLE,IO_000021,I/O Properties Checks for One I/O,The I/O standard should support the requested Weak Pull Up value.,Critical,No Weak Pull-Up Resistor assignments found.,,I/O,,
IO_RULES,IO_STD_SUPPORT_BUS_HOLD_VALUE,INAPPLICABLE,IO_000022,I/O Properties Checks for One I/O,The I/O standard should support the requested Bus Hold value.,Critical,No Enable Bus-Hold Circuitry assignments found.,,I/O,,
IO_RULES,IO_STD_SUPPORT_OPEN_DRAIN_VALUE,INAPPLICABLE,IO_000023,I/O Properties Checks for One I/O,The I/O standard should support the Open Drain value.,Critical,No open drain assignments found.,,I/O,,
IO_RULES,IO_DIR_SUPPORT_OCT_VALUE,PASS,IO_000024,I/O Properties Checks for One I/O,The I/O direction should support the On Chip Termination value.,Critical,0 such failures found.,,I/O,,
IO_RULES,OCT_AND_CURRENT_STRENGTH_NOT_USED_SIMULTANEOUSLY,INAPPLICABLE,IO_000026,I/O Properties Checks for One I/O,On Chip Termination and Current Strength should not be used at the same time.,Critical,No Current Strength assignments found.,,I/O,,
IO_RULES,WEAK_PULL_UP_AND_BUS_HOLD_NOT_USED_SIMULTANEOUSLY,INAPPLICABLE,IO_000027,I/O Properties Checks for One I/O,Weak Pull Up and Bus Hold should not be used at the same time.,Critical,No Enable Bus-Hold Circuitry or Weak Pull-Up Resistor assignments found.,,I/O,,
IO_RULES,IO_STD_SUPPORTS_SLEW_RATE,INAPPLICABLE,IO_000045,I/O Properties Checks for One I/O,The I/O standard should support the requested Slew Rate value.,Critical,No Slew Rate assignments found.,,I/O,,
IO_RULES,LOC_SUPPORTS_SLEW_RATE,INAPPLICABLE,IO_000046,I/O Properties Checks for One I/O,The location should support the requested Slew Rate value.,Critical,No Slew Rate assignments found.,,I/O,,
IO_RULES,OCT_SUPPORTS_SLEW_RATE,INAPPLICABLE,IO_000047,I/O Properties Checks for One I/O,On Chip Termination and Slew Rate should not be used at the same time.,Critical,No Slew Rate assignments found.,,I/O,,
IO_RULES,SINGLE_ENDED_OUTPUTS_LAB_ROWS_FROM_DIFF_IO,PASS,IO_000034,SI Related Distance Checks,Single-ended outputs should be 0 LAB row(s) away from a differential I/O.,High,0 such failures found.,,I/O,,
IO_RULES,DEV_IO_RULE_LVDS_DISCLAIMER,,,,,,,,,,
IO_RULES,DEV_IO_RULE_OCT_DISCLAIMER,,,,,,,,,,
IO_RULES,DEV_IO_RULE_GXB_DISCLAIMER,,,,,,,,,,
IO_RULES_MATRIX,Pin/Rules,IO_000001;IO_000002;IO_000003;IO_000004;IO_000005;IO_000006;IO_000007;IO_000008;IO_000009;IO_000010;IO_000011;IO_000012;IO_000013;IO_000014;IO_000015;IO_000018;IO_000019;IO_000020;IO_000021;IO_000022;IO_000023;IO_000024;IO_000026;IO_000027;IO_000045;IO_000046;IO_000047;IO_000034,
IO_RULES_MATRIX,Total Pass,14;0;14;0;0;33;14;0;33;33;0;23;0;0;0;0;23;0;0;0;0;23;0;0;0;0;0;24,
IO_RULES_MATRIX,Total Unchecked,0;0;0;0;0;0;0;0;0;0;0;0;0;0;0;0;0;0;0;0;0;0;0;0;0;0;0;0,
IO_RULES_MATRIX,Total Inapplicable,19;33;19;33;33;0;19;33;0;0;33;10;33;33;33;33;10;33;33;33;33;10;33;33;33;33;33;9,
IO_RULES_MATRIX,Total Fail,0;0;0;0;0;0;0;0;0;0;0;0;0;0;0;0;0;0;0;0;0;0;0;0;0;0;0;0,
IO_RULES_MATRIX,DIS_USER_CLK,Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Pass;Inapplicable;Inapplicable;Pass;Pass;Inapplicable;Pass;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Pass;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Pass;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Pass,
IO_RULES_MATRIX,DIS_TX_CLK,Pass;Inapplicable;Pass;Inapplicable;Inapplicable;Pass;Pass;Inapplicable;Pass;Pass;Inapplicable;Pass;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Pass;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Pass;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Pass,
IO_RULES_MATRIX,DIS_RX_CLK,Pass;Inapplicable;Pass;Inapplicable;Inapplicable;Pass;Pass;Inapplicable;Pass;Pass;Inapplicable;Pass;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Pass;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Pass;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Pass,
IO_RULES_MATRIX,HARD_ERR,Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Pass;Inapplicable;Inapplicable;Pass;Pass;Inapplicable;Pass;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Pass;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Pass;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Pass,
IO_RULES_MATRIX,SOFT_ERR,Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Pass;Inapplicable;Inapplicable;Pass;Pass;Inapplicable;Pass;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Pass;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Pass;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Pass,
IO_RULES_MATRIX,FRAME_ERR,Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Pass;Inapplicable;Inapplicable;Pass;Pass;Inapplicable;Pass;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Pass;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Pass;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Pass,
IO_RULES_MATRIX,ERR_COUNT[7],Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Pass;Inapplicable;Inapplicable;Pass;Pass;Inapplicable;Pass;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Pass;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Pass;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Pass,
IO_RULES_MATRIX,ERR_COUNT[6],Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Pass;Inapplicable;Inapplicable;Pass;Pass;Inapplicable;Pass;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Pass;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Pass;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Pass,
IO_RULES_MATRIX,ERR_COUNT[5],Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Pass;Inapplicable;Inapplicable;Pass;Pass;Inapplicable;Pass;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Pass;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Pass;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Pass,
IO_RULES_MATRIX,ERR_COUNT[4],Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Pass;Inapplicable;Inapplicable;Pass;Pass;Inapplicable;Pass;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Pass;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Pass;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Pass,
IO_RULES_MATRIX,ERR_COUNT[3],Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Pass;Inapplicable;Inapplicable;Pass;Pass;Inapplicable;Pass;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Pass;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Pass;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Pass,
IO_RULES_MATRIX,ERR_COUNT[2],Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Pass;Inapplicable;Inapplicable;Pass;Pass;Inapplicable;Pass;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Pass;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Pass;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Pass,
IO_RULES_MATRIX,ERR_COUNT[1],Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Pass;Inapplicable;Inapplicable;Pass;Pass;Inapplicable;Pass;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Pass;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Pass;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Pass,
IO_RULES_MATRIX,ERR_COUNT[0],Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Pass;Inapplicable;Inapplicable;Pass;Pass;Inapplicable;Pass;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Pass;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Pass;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Pass,
IO_RULES_MATRIX,LANE_UP,Pass;Inapplicable;Pass;Inapplicable;Inapplicable;Pass;Pass;Inapplicable;Pass;Pass;Inapplicable;Pass;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Pass;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Pass;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Pass,
IO_RULES_MATRIX,CHANNEL_UP,Pass;Inapplicable;Pass;Inapplicable;Inapplicable;Pass;Pass;Inapplicable;Pass;Pass;Inapplicable;Pass;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Pass;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Pass;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Pass,
IO_RULES_MATRIX,RXN,Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Pass;Inapplicable;Inapplicable;Pass;Pass;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable,
IO_RULES_MATRIX,TXP,Pass;Inapplicable;Pass;Inapplicable;Inapplicable;Pass;Pass;Inapplicable;Pass;Pass;Inapplicable;Pass;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Pass;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Pass;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Pass,
IO_RULES_MATRIX,TXN,Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Pass;Inapplicable;Inapplicable;Pass;Pass;Inapplicable;Pass;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Pass;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Pass;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Pass,
IO_RULES_MATRIX,GXB_DOWN,Pass;Inapplicable;Pass;Inapplicable;Inapplicable;Pass;Pass;Inapplicable;Pass;Pass;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable,
IO_RULES_MATRIX,RXP,Pass;Inapplicable;Pass;Inapplicable;Inapplicable;Pass;Pass;Inapplicable;Pass;Pass;Inapplicable;Pass;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Pass;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Pass;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Pass,
IO_RULES_MATRIX,GTXQ4,Pass;Inapplicable;Pass;Inapplicable;Inapplicable;Pass;Pass;Inapplicable;Pass;Pass;Inapplicable;Pass;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Pass;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Pass;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Pass,
IO_RULES_MATRIX,INIT_CLK,Pass;Inapplicable;Pass;Inapplicable;Inapplicable;Pass;Pass;Inapplicable;Pass;Pass;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable,
IO_RULES_MATRIX,RESET,Pass;Inapplicable;Pass;Inapplicable;Inapplicable;Pass;Pass;Inapplicable;Pass;Pass;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable,
IO_RULES_MATRIX,GT_RESET_IN,Pass;Inapplicable;Pass;Inapplicable;Inapplicable;Pass;Pass;Inapplicable;Pass;Pass;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable,
IO_RULES_MATRIX,altera_reserved_tms,Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Pass;Inapplicable;Inapplicable;Pass;Pass;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable,
IO_RULES_MATRIX,altera_reserved_tck,Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Pass;Inapplicable;Inapplicable;Pass;Pass;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable,
IO_RULES_MATRIX,altera_reserved_tdi,Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Pass;Inapplicable;Inapplicable;Pass;Pass;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable,
IO_RULES_MATRIX,altera_reserved_ntrst,Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Pass;Inapplicable;Inapplicable;Pass;Pass;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable,
IO_RULES_MATRIX,altera_reserved_tdo,Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Pass;Inapplicable;Inapplicable;Pass;Pass;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Pass,
IO_RULES_MATRIX,TXP(n),Pass;Inapplicable;Pass;Inapplicable;Inapplicable;Pass;Pass;Inapplicable;Pass;Pass;Inapplicable;Pass;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Pass;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Pass;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Pass,
IO_RULES_MATRIX,RXP(n),Pass;Inapplicable;Pass;Inapplicable;Inapplicable;Pass;Pass;Inapplicable;Pass;Pass;Inapplicable;Pass;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Pass;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Pass;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Pass,
IO_RULES_MATRIX,GTXQ4(n),Pass;Inapplicable;Pass;Inapplicable;Inapplicable;Pass;Pass;Inapplicable;Pass;Pass;Inapplicable;Pass;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Pass;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Pass;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Inapplicable;Pass,
IO_RULES_SUMMARY,Total I/O Rules,28,
IO_RULES_SUMMARY,Number of I/O Rules Passed,10,
IO_RULES_SUMMARY,Number of I/O Rules Failed,0,
IO_RULES_SUMMARY,Number of I/O Rules Unchecked,0,
IO_RULES_SUMMARY,Number of I/O Rules Inapplicable,18,
